Month/Year: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/ \_\_\_\_\_\_\_\_\_

Workers Inspected: Deficiency Deficiency

Yes No Yes No

1. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

3. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

4. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Comments: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*Add inspectors initials in the box below corresponding to the date of the month the PPE is inspected.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Day of Month | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16 |
| Initial |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Day of Month | 17 | 18 | 19 | 20 | 21 | 22 | 23 | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31 |  |
| Initial |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Inspection Criteria:

1. *CSA Approved Steel Toe Boot*

* CSA Standard Z195
* No Exposed Steel Toe, holes, cracks
* Green Triangle & White Tag
* Non-Slip Tread & Intact

2*. CSA Approved Safety Glasses*

* CSA Standard Z94.3
* Fit close to face & around eyes
* Clean & no scratches in vision
* Glasses to go over top or prescription glasses

3. *Gloves*

* No holes or loose fibers
* Suited for the task performed

4. *CSA Approved High Visibility*

* CSA Standard Z96-15
* Clean, vibrant, no worn reflective material

*5. CSA Approved Hearing Protection*

* CSA Standard Z94.2
* Clean & Hair or clothing not in the way
* Tightly seals within the ear canal or against the side of the head

6. *CSA Approved Respirator or Mask*

* CSA Standard Z94.4
* No cracks, tears, missing, worn, broken parts
* Fits close to face
* Correct Cartridges used
* Respirator checklist used

7. CSA Work Positioning System

* ANSI Z133.1 - 2000
* Correct type used for work performed
* Rescue plan in place
* Formally trained to use system – check card
* Serviced within last year
* Hanging when not used

8. CSA Approved Head Protection

* CSA Standard Z94.1
* Wear, scratches, gouges, hairline cracks