Worker Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Scope of Work: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Weather Conditions: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Validation Period: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/\_\_\_\_/\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/\_\_\_\_/\_\_\_\_\_\_\_

**Inspection Procedure:**

Use the Work Positioning System Checklist before wearing work positioning systems to inspect saddle, lanyard, shock absorber, D-Rings, connecting links, climbing lines, and spurs. See Tree Care Guidelines for more information.

**Potential Fall Hazards:**



**Tools Required:**



**Aerial Rescue Plan:**

1. Use of an aerial platform to collect fallen worker, disconnect system, and bring to ground.
2. Use a rescuer to connect, ascend, collect worker, and descend to the ground.
3. Use of a ladder to support fallen worker, disconnect system, and guide down the ladder, if conscious.

**\*All workers suffering a fall from height must seek medical attention as soon as reasonably possible.**

|  |  |  |
| --- | --- | --- |
| Print Name | Signature | Trained in Aerial Rescue.  (Yes or No) |
|  |  |  |
|  |  |  |
|  |  |  |

⃞ Work Positioning System checklist for each system used, completed and attached.